Ergonomic design to ensure low differential pressure or no turbulence in high flow fluid systems to 250g per min
Integrated cleaning mechanism for easy ferrous material removal for further diagnostics
External fitting format for easy in-field installation and application across all medium to small equipment types
Highest quality materials and manufacturing methods to ensure it lasts the life of the asset
Proprietary design incorporating top quality and high capacity rod style rare earth magnets to capture and hold more