Innovative design ensures low pressure drops at flow rates up to 350 L/min
External fitting format for easy in-field installation and application across all medium to small equipment types
Integrated cleaning mechanism for easy ferrous material removal for further diagnostics
Proprietary design incorporating high quality rod style rare earth magnets that can capture and hold up to 264g of ferrous material
Highest quality materials and manufacturing methods to ensure it lasts the life of the asset